; Description: Bulgarian Language, Phonetic layout keyboard WWE (QWERTY); Date: 28.04.2006
; Adapted by: Antoni Ivanov (prezimir@gmail.com)
; CapsLock fix: Milen Boev 23.1.2007 (mentox@abv.bg)
; Please note that parameters in this file should be in the same order as described.
; 
; Keyboard layout name (displayed in AEKMapSettings)
Layout Bulgarian (Phonetic) - mentox

; Hint for the layout to be shown in lower right corner of the screen
Hint BG
CapslockKey 0014 0114
; Tips (mentox):
; switching 007A = Dot + Space
; default Hint text: EN


; "Hardware" parameter adjust keyboard processing algoritm to 
; specific hardware. Most of the keyboards will work with default 
; settings (no Hardware parameter or empty), but specifying 
; correct hardware platform may help you to resolve some issues
; Valid values and AEKMap versions are:
;
; Wizard
;   "HTC Wizard" is a device sold by many brands under different names:
;   O2 XDA Mini S / I-Mate K-Jam / Qtek 9100 / T-Mobile MDA Vario /
;   Orange SPV M3000 / Dopod 838 / Vodafone VPA Compact II
;   Specifying Wizard as hardware platform will allow AEKMap to distinguish 
;   joystik and Enter/Arrows on hardware keyboard.
;   Requires AEKMap v1.1.3 or later.
;
Hardware Wizard

; Key Mappings

; A
Key 0141 c0410 ; ShiftA -> À
Key 0041 c0430 ; A -> à

; B
Key 0142 c0411 ; ShiftB -> Á
Key 0042 c0431 ; B -> á

; C
Key 0143 c0426 ; ShiftC -> Ö
Key 0043 c0446 ; C -> ö

; D
Key 0144 c0414 ; ShiftD -> Ä
Key 0044 c0434 ; D -> Ä

; E
Key 0145 c0415 ; ShiftE -> Å
Key 0045 c0435 ; E -> å

; F
Key 0146 c0424 ; ShiftF -> Ô
Key 0046 c0444 ; F -> ô

; G
Key 0147 c0413 ; ShiftG -> Ã
Key 0047 c0433 ; G -> ã

; H
Key 0148 c0425 ; ShiftH -> Õ
Key 0048 c0445 ; H -> õ

; I
Key 0149 c0418 ; ShiftI -> È
Key 0049 c0438 ; I -> è

; J
Key 014A c0419 ; ShiftJ -> É
Key 004A c0439 ; J -> é

; K
Key 014B c041A ; ShiftK -> Ê
Key 004B c043A ; K -> ê

; L
Key 014C c041B ; ShiftL -> Ë
Key 004C c043B ; L -> ë

; M
Key 014D c041C ; ShiftM -> Ì
Key 004D c043C ; M -> ì

; N
Key 014E c041D ; ShiftN -> Í
Key 004E c043D ; N -> í

; O
Key 014F c041E ; ShiftO -> Î
Key 004F c043E ; O -> î

; P
Key 0150 c041F ; ShiftP -> Ï
Key 0050 c043F ; P -> ï

; Q
Key 0151 c042F ; ShiftQ -> ß
Key 0051 c044F ; Q -> ÿ

; R
Key 0152 c0420 ; ShiftR -> Ð
Key 0052 c0440 ; R -> ð

; S
Key 0153 c0421 ; ShiftS -> Ñ
Key 0053 c0441 ; S -> ñ

; T
Key 0154 c0422 ; ShiftT -> Ò
Key 0054 c0442 ; T -> ò

; U
Key 0155 c0423 ; ShiftU -> Ó
Key 0055 c0443 ; U -> ó

; V
Key 0156 c0416 ; ShiftV -> Æ
Key 0056 c0436 ; V -> æ

; W
Key 0157 c0412 ; ShiftW -> Â
Key 0057 c0432 ; W -> â

; X
Key 0158 c042C ; ShiftX -> Ü
Key 0058 c044C ; X -> ü

; Y
Key 0159 c042A ; ShiftY -> Ú
Key 0059 c044A ; Y -> ú

; Z
Key 015A c0417 ; ShiftZ -> Ç
Key 005A c0437 ; Z -> ç

; Additional cyrrilic letters used in Bulgarian

; Up Arrow
Key 0126 c042E ; ShiftUp -> Þ
Key 0026 c044E ; Up -> þ

; Left Arrow
Key 0125 c0427 ; ShiftLeft -> ×
Key 0025 c0447 ; Left -> ÷

; DOwn Arrow
Key 0128 c0428 ; ShiftDown -> Ø
Key 0028 c0448 ; Down -> ø

; Right Arrow
Key 0127 c0429 ; ShiftRight -> Ù
Key 0027 c0449 ; Right -> ù
